<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="7.027" y1="0.8" x2="127.027" y2="0.8" width="0" layer="20"/>
<wire x1="127.027" y1="0.8" x2="127.027" y2="100.8" width="0" layer="20"/>
<wire x1="127.027" y1="100.8" x2="7.027" y2="100.8" width="0" layer="20"/>
<wire x1="7.027" y1="100.8" x2="7.027" y2="0.8" width="0" layer="20"/>
<hole x="121.497" y="6.35" drill="3"/>
<hole x="121.497" y="95.25" drill="3"/>
<hole x="31.497" y="95.25" drill="3"/>
<hole x="31.497" y="6.35" drill="3"/>
<text>LC-Meter V 1.0 (c)
05/2014 by DL8NCI</text>
<text>LC-Meter V 1.0 (c)
05/2014 by DL8NC</text>
<text>LC-Meter-Proto-131.brd</text>
<text>LC-Meter-Proto-131.brd</text>
<text>+5V</text>
<text>SDA</text>
<text>SCL</text>
<text>-INT</text>
<text>GND</text>
<text>+5V</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P6</text>
<text>P2</text>
<text>P7</text>
<text>ZRO-LED</text>
<text>GND</text>
<text>+5V</text>
<text>GND</text>
<text>ADC7</text>
<text>ADC6</text>
<text>ADC5</text>
<text>ADC4</text>
<text>ADC3</text>
<text>ADC2</text>
<text>PD4/OC1B</text>
<text>PB3/AIN1</text>
<text>LC-Meter V1.0
(c) 05/2014
by DL8NCI</text>
<text>GND</text>
<text>RESET</text>
<text>solder side</text>
<text>component side</text>
<text>ZRO_KEY</text>
<text>LC-Meter-Proto-131.brd</text>
</plain>
<libraries>
<library name="zavr">
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="SMCC">
<description>SMCC</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="E2-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.0 mm, diameter 6 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="SPEZIAL1">
<description>Gedacht für verschiedene Bestückungsvarianten für 330 pF:&lt;br&gt;
&lt;a href = 'http://www.reichelt.de/Wima-FKS2-FKC2-FKP2/FKP-2-1000-330P/3/index.html?&amp;ACTION=3&amp;LA=2&amp;ARTICLE=31952&amp;GROUPID=3151&amp;artnr=FKP-2-1000+330P'&gt;WIMA FKP-2, 2.5%, 1000 V, 5 mm&lt;/a&gt;&lt;br&gt;
&lt;a href='http://www.reichelt.de/Styroflexkondensatoren/STYROFLEX-330P/3/index.html?&amp;ACTION=3&amp;LA=2&amp;ARTICLE=19851&amp;GROUPID=3158&amp;artnr=STYROFLEX+330P'&gt;Styroflex, 2%, 4.5 x 11.5 mm&lt;/a&gt;&lt;br&gt;
&lt;a href = 'http://www.reichelt.de/Styroflexkondensatoren/CY-22-3-330P/3/index.html?&amp;ACTION=3&amp;LA=2&amp;ARTICLE=42436&amp;GROUPID=3158&amp;artnr=CY+22-3+330P'&gt;Glimmer, 2%, 100 V, 4.5 mm&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="zatmel">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="relay">
<packages>
<package name="HE3621">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, grid 5.08 mm, Hamlin</description>
</package>
</packages>
</library>
<library name="zSonstiges">
<packages>
<package name="V_PR18/25">
<description>Kühlkörper Reichelt V PR18/25 - 17 K/W</description>
</package>
<package name="700460">
<description>Drucktaster MTS602</description>
</package>
<package name="UM2102">
<description>Elektor Modul UM2102&lt;br&gt;
SER nach USB&lt;br&gt;
änlich FT232</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="zv-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78LXX-1">
<description>78LXX - Beinchen in einer Reihe - eng</description>
</package>
</packages>
</library>
<library name="micro-philips">
<description>&lt;b&gt;Philips Microcontroller Devices&lt;/b&gt;&lt;p&gt;
http://www-eu2.semiconductors.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-pss254_reichelt">
<description>Reichelt Einzelstecker Raster 2,54mm
PSS 254</description>
<packages>
<package name="05G">
</package>
<package name="10G">
</package>
<package name="02G">
</package>
</packages>
</library>
<library name="con-lumberg">
<packages>
<package name="NEB1R-SPEZIAL">
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE05-1">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="zLCD">
<packages>
<package name="ML14">
</package>
</packages>
</library>
<library name="resistor-net">
<description>&lt;b&gt;Generic Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RN-5">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="zavr" package="DIL40" value="ATmega32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="ATMEGA 32-16 DIP"/>
</element>
<element name="Q1" library="crystal" package="HC49/S" value="14.7456 MHz">
<attribute name="NAME"/>
<attribute name="REICHELT" value="14,7456-HC18"/>
</element>
<element name="C1" library="rcl" package="C025-025X050" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="KERKO 22P"/>
</element>
<element name="C2" library="rcl" package="C025-025X050" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="KERKO 22P"/>
</element>
<element name="C3" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="C4" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="C5" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="C6" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="L1" library="rcl" package="SMCC" value="10µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="SMCC 10µ"/>
</element>
<element name="L2" library="rcl" package="SMCC" value="47µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="SMCC 47µ"/>
</element>
<element name="C7" library="rcl" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="TANTAL 10/16"/>
</element>
<element name="J2" library="zatmel" package="2X03" value="ISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MPE 087-2-006"/>
</element>
<element name="C8" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="IC2" library="linear" package="DIL08" value="LM311">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="LM 311 DIP"/>
</element>
<element name="R4" library="rcl" package="0207/10" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="METALL 100K"/>
</element>
<element name="R5" library="rcl" package="0207/10" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="METALL 100K"/>
</element>
<element name="R6" library="rcl" package="0207/10" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="METALL 1,00K"/>
</element>
<element name="R7" library="rcl" package="0207/10" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="METALL 47,0K"/>
</element>
<element name="R3" library="rcl" package="0207/10" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="METALL 100K"/>
</element>
<element name="C9" library="rcl" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="TANTAL 10/16"/>
</element>
<element name="C10" library="rcl" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="TANTAL 10/16"/>
</element>
<element name="C11" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="C12" library="rcl" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="TANTAL 10/16"/>
</element>
<element name="C13" library="rcl" package="C050-055X075" value="470p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="FKP-2-1000 470P"/>
</element>
<element name="L3" library="rcl" package="SMCC" value="47µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="SMCC 47µ"/>
</element>
<element name="IC3" library="linear" package="DIL08" value="NE555">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="NE 555 DIP"/>
</element>
<element name="C16" library="rcl" package="C025-025X050" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 10N"/>
</element>
<element name="R8" library="rcl" package="0207/5V" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MPR 1,00M"/>
</element>
<element name="R9" library="rcl" package="0207/5V" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MPR 33,0K"/>
</element>
<element name="R10" library="rcl" package="0207/5V" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MPR 1,00K"/>
</element>
<element name="C18" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="C19" library="rcl" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="TANTAL 10/16"/>
</element>
<element name="R2" library="rcl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="METALL 10,0K"/>
</element>
<element name="C23" library="rcl" package="C025-025X050" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 10N"/>
</element>
<element name="C24" library="rcl" package="E2-6" value="22uF">
<attribute name="REICHELT" value="RAD 22/25"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C050-030X075" value="330n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MKS-2 330N"/>
</element>
<element name="C26" library="rcl" package="C050-030X075" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MKS-2 100N"/>
</element>
<element name="D3" library="diode" package="DO41-10" value="1N4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="1N 4001"/>
</element>
<element name="K1" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="K2" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="K4" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="K5" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="K6" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="K7" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="C20" library="rcl" package="C050-030X075" value="330n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MKS-2 330N"/>
</element>
<element name="C21" library="rcl" package="C050-030X075" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="MKS-2 100N"/>
</element>
<element name="IC4" library="v-reg" package="78XXL" value="7805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="µA 7805"/>
</element>
<element name="KK1" library="zSonstiges" package="V_PR18/25" value="">
<attribute name="REICHELT" value="V PR18/25"/>
</element>
<element name="D2" library="diode" package="DO41-10" value="1N4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="1N 4001"/>
</element>
<element name="K8" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="K3" library="relay" package="HE3621" value="">
<attribute name="OC_NEWARK" value="50F7993"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="MF" value="HAMLIN"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 7271-D 5V"/>
</element>
<element name="IC5" library="zv-reg" package="78LXX-1" value="78L05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="µA 78L05"/>
</element>
<element name="D4" library="diode" package="DO41-10" value="1N4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="1N 4001"/>
</element>
<element name="D5" library="diode" package="DO41-10" value="1N4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="1N 4001"/>
</element>
<element name="IC6" library="micro-philips" package="DIL16" value="PCF8574P">
<attribute name="OC_NEWARK" value="11N8515"/>
<attribute name="MPN" value="PCF8574PN"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="204020"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="PCF 8574 P"/>
</element>
<element name="C15" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="IC7" library="micro-philips" package="DIL16" value="PCF8574P">
<attribute name="OC_NEWARK" value="11N8515"/>
<attribute name="MPN" value="PCF8574PN"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="204020"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="PCF 8574 P"/>
</element>
<element name="C17" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="S1" library="zSonstiges" package="700460" value="700460">
<attribute name="NAME"/>
<attribute name="CONRAD" value="700460"/>
<attribute name="REICHELT" value="TASTER 9302"/>
</element>
<element name="D1" library="diode" package="DO41-10" value="1N4001">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="1N 4001"/>
</element>
<element name="J3" library="con-pss254_reichelt" package="05G" value="I2C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="PSS 254/5G"/>
</element>
<element name="J4" library="con-pss254_reichelt" package="10G" value="AUX2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="PSS 254/10G"/>
</element>
<element name="J5" library="con-pss254_reichelt" package="10G" value="AUX1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="PSS 254/10G"/>
</element>
<element name="J6" library="con-pss254_reichelt" package="02G" value="Lx/Cx">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="PSS 254/2G"/>
</element>
<element name="C14" library="rcl" package="SPEZIAL1" value="330p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="FKP-2-1000 330P"/>
</element>
<element name="J7" library="con-lumberg" package="NEB1R-SPEZIAL" value="NEB1R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="LUM NEB 1R"/>
</element>
<element name="M1" library="zSonstiges" package="UM2102" value="UM2102">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="ELV" value="68-09 18 59"/>
</element>
<element name="C22" library="rcl" package="C025-025X050" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="Z5U-2,5 100N"/>
</element>
<element name="J8" library="con-lsta" package="FE05-1" value="NIBOBee Blue">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="NIBO BEE BLUE"/>
</element>
<element name="J1" library="zLCD" package="ML14" value="OLED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="REICHELT" value="WSL 14G"/>
</element>
<element name="R1" library="resistor-net" package="RN-5" value="4k7">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="REICHELT" value="SIL 5-4 4,7K"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="32"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="L1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$8">
<contactref element="L2" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="+5V">
<contactref element="L2" pad="1"/>
<contactref element="C7" pad="+"/>
<contactref element="C5" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="C19" pad="+"/>
<contactref element="C18" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="K1" pad="2"/>
<contactref element="K2" pad="2"/>
<contactref element="K4" pad="2"/>
<contactref element="K5" pad="2"/>
<contactref element="K6" pad="2"/>
<contactref element="K7" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="IC4" pad="OUT"/>
<contactref element="D2" pad="C"/>
<contactref element="K8" pad="2"/>
<contactref element="K3" pad="2"/>
<contactref element="K4" pad="4"/>
<contactref element="K5" pad="4"/>
<contactref element="K6" pad="4"/>
<contactref element="IC6" pad="16"/>
<contactref element="C15" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC7" pad="16"/>
<contactref element="C17" pad="1"/>
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="10"/>
<contactref element="J5" pad="10"/>
<contactref element="C22" pad="2"/>
<contactref element="J8" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="J2" pad="5"/>
<contactref element="IC1" pad="9"/>
<contactref element="R2" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="N$51">
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$52">
<contactref element="IC2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="N$55">
<contactref element="IC2" pad="3"/>
<contactref element="C10" pad="+"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="C13" pad="1"/>
<contactref element="L3" pad="2"/>
<contactref element="C9" pad="-"/>
<contactref element="K1" pad="1"/>
<contactref element="K2" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="L3" pad="1"/>
<contactref element="K1" pad="4"/>
<contactref element="K7" pad="1"/>
<contactref element="K3" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="C16" pad="2"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="NE555_C">
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="6"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="K8" pad="1"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="N$87">
<contactref element="D1" pad="A"/>
<contactref element="J7" pad="CTR@2"/>
<contactref element="J7" pad="CTR@1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="C24" pad="+"/>
<contactref element="C25" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="C20" pad="1"/>
<contactref element="IC4" pad="IN"/>
<contactref element="IC5" pad="IN"/>
<contactref element="D4" pad="C"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$85">
<contactref element="R5" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="R6" pad="2"/>
<contactref element="C12" pad="+"/>
<contactref element="C11" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="IC5" pad="OUT"/>
<contactref element="D4" pad="A"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="REL_1K">
<contactref element="K4" pad="3"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="REL_33K">
<contactref element="K5" pad="3"/>
<contactref element="IC6" pad="11"/>
</signal>
<signal name="REL_1MEG">
<contactref element="K6" pad="3"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="NE555_TRIG">
<contactref element="IC1" pad="19"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="NE555_OUT">
<contactref element="IC1" pad="20"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="LCD_R/-W">
<contactref element="IC1" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="LCD_RS">
<contactref element="IC1" pad="3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="LCD_E">
<contactref element="IC1" pad="24"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="PC4">
<contactref element="IC1" pad="26"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="PC5">
<contactref element="IC1" pad="27"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="PC6">
<contactref element="IC1" pad="28"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="PC7">
<contactref element="IC1" pad="29"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="PB5">
<contactref element="IC1" pad="6"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="PB6">
<contactref element="IC1" pad="7"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="PB7">
<contactref element="IC1" pad="8"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="LM311_OUT">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="REL_L3">
<contactref element="K1" pad="3"/>
<contactref element="IC6" pad="4"/>
</signal>
<signal name="REL_330P">
<contactref element="K2" pad="3"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="REL_LX">
<contactref element="K7" pad="3"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="K8" pad="4"/>
<contactref element="K3" pad="4"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="REL_LM311">
<contactref element="K3" pad="3"/>
<contactref element="IC6" pad="12"/>
</signal>
<signal name="N$9">
<contactref element="K6" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="K5" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="K4" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="K2" pad="4"/>
<contactref element="C14" pad="1B"/>
<contactref element="C14" pad="1A"/>
<contactref element="C14" pad="1C"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="15"/>
<contactref element="M1" pad="2.3"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="14"/>
<contactref element="M1" pad="2.2"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="0V">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="-"/>
<contactref element="C6" pad="2"/>
<contactref element="IC1" pad="11"/>
<contactref element="J2" pad="6"/>
<contactref element="C8" pad="2"/>
<contactref element="IC1" pad="31"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="-"/>
<contactref element="C25" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="IC4" pad="GND"/>
<contactref element="D2" pad="A"/>
<contactref element="IC2" pad="1"/>
<contactref element="C10" pad="-"/>
<contactref element="IC2" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="-"/>
<contactref element="C13" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C19" pad="-"/>
<contactref element="C18" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="K7" pad="4"/>
<contactref element="IC5" pad="GND"/>
<contactref element="D5" pad="A"/>
<contactref element="IC1" pad="40"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC6" pad="2"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="8"/>
<contactref element="C15" pad="2"/>
<contactref element="IC7" pad="2"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC7" pad="8"/>
<contactref element="C17" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="C14" pad="2B"/>
<contactref element="C14" pad="2A"/>
<contactref element="C14" pad="2C"/>
<contactref element="J7" pad="OUT"/>
<contactref element="J7" pad="2"/>
<contactref element="M1" pad="2.4"/>
<contactref element="C22" pad="1"/>
<contactref element="J8" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="ADC7">
<contactref element="IC1" pad="33"/>
<contactref element="J5" pad="9"/>
</signal>
<signal name="ADC5">
<contactref element="IC1" pad="35"/>
<contactref element="J5" pad="7"/>
</signal>
<signal name="NE555_RESET">
<contactref element="IC3" pad="4"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="AIN1">
<contactref element="IC1" pad="4"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="ADC3">
<contactref element="IC1" pad="37"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="IC6" pad="15"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC7" pad="15"/>
<contactref element="J3" pad="3"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="IC6" pad="14"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC7" pad="14"/>
<contactref element="J3" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="REL_NE555">
<contactref element="K8" pad="3"/>
<contactref element="IC6" pad="10"/>
</signal>
<signal name="P1/ZERO_LED">
<contactref element="IC7" pad="5"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="P2">
<contactref element="IC7" pad="6"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="P3">
<contactref element="IC7" pad="7"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="P6">
<contactref element="IC7" pad="11"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="P5">
<contactref element="IC7" pad="10"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="P4">
<contactref element="IC7" pad="9"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="ADC2">
<contactref element="IC1" pad="38"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="ADC4">
<contactref element="IC1" pad="36"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="ADC6">
<contactref element="IC1" pad="34"/>
<contactref element="J5" pad="8"/>
</signal>
<signal name="P7">
<contactref element="IC7" pad="12"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="PD4">
<contactref element="IC1" pad="18"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="N$26">
<contactref element="IC1" pad="16"/>
<contactref element="IC7" pad="13"/>
<contactref element="R1" pad="5"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="P0/ZERO_KEY">
<contactref element="IC7" pad="4"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="VO">
<contactref element="J1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
